=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Jan-2011
La Gomera is a new station first data 2007 and forms part of the newly established REDMAR
network.Gauge is a MIROS radar sensor. Benchmark S/N is 2.899m relative to the REDMAR datum and
1.431m to IGN.
See paper B. Perez et al 'Overlapping sea level time series measured using different technologies:
an example from the REDMAR Spanish network'.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Apr-2014
At the request of Puertos del Estado the latitude and longitude for this station has been revised from 28.086667 -17.108333 derived from the previously supplied degrees and minutes value  to 28.08777 -17.10831 which is the position of the new MIROS gauge in decimal degrees.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Jul-2025
This station revealed very local movements of the quay, so this data should be used with care. The supplier is reviewing the levelling information and GNSS data and will provide more details as soon as available.

